/ Title: Spar buoy definitions - cylindirical and spherical
/ PLDYN test input file: SI units [m,N,sec]

/ Copyright 2021 Ibrahim Konuk
/ model number =<100>=
/ filename = pldynS3_buoy.pi

 set_param(echo_OFF);


flow_director(to_output="Spar buoy definitions - cylindirical and spherical");
flow_director(to_console="Spar buoy definitions - cylindirical and spherical");


 BUOY_CLASS(
/-------------------------------------------
 LABEL ="PLET_Sphere",
/-------------------------------------------
                  CLASS_NUMBER = 101      ,
                     BUOY_TYPE = 1        ,
 		  BUOY_SPACING = 5.0      ,
                      DIAMETER = 1.2      ,
                        HEIGHT = 2.0      ,
                        OFFSET = 2.5      ,
                    DRY_WEIGHT = 750      ,
                          DRAG = 3750.0   , 
                       INERTIA = 3450.0   ,  
                 MINIMUM_FORCE = -750.0   ,
                 MAXIMUM_FORCE = 2500.0   );
/-------------------------------------------
/ Total value fields =<9>=
/ Total alpha fields =<1>=
/ Total key fields   =<1>=

 BUOY_CLASS(
/-------------------------------------------
 LABEL ="Cylinder",
/-------------------------------------------
                  CLASS_NUMBER = 102      ,
                     BUOY_TYPE = 2        ,
 		  BUOY_SPACING = 5.0      ,
                      DIAMETER = 1.24     ,
                        HEIGHT = 2.0      ,
                        OFFSET = 2.5      ,
                    DRY_WEIGHT = 750      ,
                          DRAG = 3750.0   , 
                       INERTIA = 3450.0   ,  
                 MINIMUM_FORCE = -750.0   ,
                 MAXIMUM_FORCE = 2500.0   );
/ Total value fields =<9>=
/ Total alpha fields =<1>=
/ Total key fields   =<1>=


 set_param(echo_OFF);
 file_operation(close);

/- end of file

