// PLDYNA commands to execute examples
// Copyright 2022 ibrahim konuk


S series:

file_operation(open,FILE_NAME=pldynS1_combocircl);	//- S&D ok [articulated stinger with regular currents]
file_operation(open,FILE_NAME=pldynS1a_combocircl);	//- S&D ok [fixed stinger withseabed slope of 5 Degree]

file_operation(open,FILE_NAME=pldynS2_combocircl);

file_operation(open,FILE_NAME=pldynS3_combocircl);
file_operation(open,FILE_NAME=pldynS3_comboeuler);
file_operation(open,FILE_NAME=pldynS3a_comboeuler);

file_operation(open,FILE_NAME=pldynS5_combocircl);	//- fixed circle with higher drag coefficients
file_operation(open,FILE_NAME=pldynS5a_combocircl);	//- fixed circle barge offset and realigned
file_operation(open,FILE_NAME=pldynS5a_comboeuler);	//- fixed euler barge offset and realigned

file_operation(open,FILE_NAME=pldynS6_combocircl);	//- fixed circle laying to Circle curve of rad 3000 m
file_operation(open,FILE_NAME=pldynS6a_combocircl);	//- fixed circle laying to Euler curve of rad 1500 m
file_operation(open,FILE_NAME=pldynS6b_combocircl);	//- fixed circle laying to Euler without currents
file_operation(open,FILE_NAME=pldynS6c_combocircl);	//- fixed circle laying to Circle without currents