/ Title: PLDYNA typical control parameters
/ PLDYN test input file: SI units [m,N,sec]

/ Copyright 2021 Ibrahim Konuk
/ model number =<100>=
/ filename = pldyn8S3_control.pi

 set_param(echo_OFF);


flow_director(to_output="PLDYNA typical control parameters");
flow_director(to_console="PLDYNA typical control parameters");


 CONTROL_SET(
/-------------------------------------------
 LABEL ="DEFAULT",
/-------------------------------------------
                   CONTROL_SET = 100      ,
              MODEL_GENERATION = 3        ,
             ACCURACY_EXPONENT = 4        ,
                    ITERATIONS = 125      ,
              TOTAL_TIME_STEPS = 700      ,
             FIRST_OUTPUT_STEP = 400      ,
               OUTPUT_AT_STEPS = 4        ,
                     TIME_STEP = 0.05     ,
                  RAMPING_TIME = 20.000   ,
             DEBUG_INFORMATION = 0        ,
             ROLLER_ADJUSTMENT = 0        );
/-------------------------------------------
/ Total value fields =<10>=
/ Total alpha fields =<1>=
/ Total key fields   =<1>=


 OPTIMIZATION_DATA(
/-------------------------------------------
 LABEL ="NO#OPTIMIZATION",
/-------------------------------------------
              OPTIMIZATION_SET = 100      ,
             OPTIMIZATION_MODE = 1        ,
            VARIABLE_PARAMETER = 4        ,
              TARGET_PARAMETER = 2        ,
                 TARGET_ROLLER = 14       ,
                  TARGET_VALUE = 1.500e+07,
                 TARGET_STRESS = 0.700    ,
                TARGET_TENSION = 2.100e+07);
/-------------------------------------------
/ Total value fields =<9>=
/ Total alpha fields =<1>=
/ Total key fields   =<1>=


 set_param(echo_OFF);
 file_operation(close);

/- end of file

